Polarization supply for multi channel ion detector

N.Lupsa, V.Mirel, N.Partoc

National Institute for Research and Development of Isotopic and Molecular Technologies, Cluj-Napoca, RO-400293, ROMANIA

The source designed and built in INCDTIM offers all the reacquired potentials  for the multi channel  ion detector. The detector can record positive and negative ions. All the generated potentials are adjustable in order to optimize the function of the detector in different situations. The setting and measuring of each potential is digitally controlled.